expand / Mounting tools

Mounting rail adapter for e.Guard RCM B 035

This adapter can be used to mount residual current monitors from the series e.Guard RCM B 035 on 35 mm mounting rails.

Installation type: Mounting rail (35 mm)
Dimensions of transformer opening: W 99 mm × H 104 mm × D 3 mm

Factory: Doepke or similar
Item designation: RCM Mount B 035
Order number: 09344935
selected make/type: ___________/___________