expand / Mounting tools

Mounting rail adapter for e.Guard RCM B 070

This adapter can be used to mount residual current monitors from the series e.Guard RCM B 070 on 35 mm mounting rails.

Installation type: Mounting rail (35 mm)
Dimensions of transformer opening: W 104 mm × H 134 mm × D 3 mm

Factory: Doepke or similar
Item designation: RCM Mount B 070
Order number: 09344945
selected make/type: ___________/___________