switch / Switch-disconnectors

switch-disconnectors,  20 A, 3 NO

switch-disconnectors
double-sided two-tier terminals for large conductor cross-section and busbar
Switch position indicator
step function when switching on

load circuit (load disconnect contact):
3 NO
Number of poles (total): 3
Rated voltage (AC): 240 V, 415 V
Rated current AC (typ.): 20 A 
Rated frequency: 50 Hz, 60 Hz
Rated insulation voltage: 690 V 

lift terminal, captive top, bottom (load circuit):
Clamping area: min. 2.5 mm² ... max. 50 mm²

Certifications: VDE
Design requirements/Standards: EN 60947-1, EN 60947-3, EN 60669-1, EN 60669-2-4, VDE 0632

Factory: Doepke or similar
Item designation: RH 020-300
Order number: 09981088
selected make/type: ___________/___________