expand / Wiring components

Busbar for DRCBO 4 type B/B+, fork, 4-pole, 16 mm², 8.5 MW (module width), 80 A

DRCBO 4-busbars For RCCB/MCB combinations DRCBO 4 type B and B+
Specification connection: fork
Module widths: 8.5
Phase arrangement: L1, L2, L3, N, L1, L2, L3, N
Rail cross-section: 16 mm²
Modular dimension, rail: 17.8
Length: 152 mm
Rated voltage AC (fix): 480 V
Rated current AC (typ.): 80 A
Neutral conductor existent

Factory: Doepke or similar
Item designation: BG4.2.16
Order number: 09920159
selected make/type: ___________/___________